

**Hardwood Maintenance (Solid & Engineered)**

Proper humidity control is essential in maintaining your new hardwood floor. This is to prevent any potential gapping and cracks.

* 35% – 55% relative humidity and a temperature of 20 degrees are ideal. Humidifiers can help in maintaining a constant temperature

A few tips:

* Regularly sweep or vacuum the floor and use a hardwood recommended cleanser
* Never pour cleaner directly on your floor
* Household cleaners, wax and oil based detergents are not recommended and can dull or damage the finish
* Clean up spills immediately
* Use felt protectors on furniture to prevent scratches, do not use plastic
* Do not wet mop your floor
* Do not move heavy furniture/appliances without proper floor protection

We recommend visiting the manufactures website for specific details on care and warranty for your new hardwood floor.