

**Laminate Maintenance**

Following installation, clean with a recommended no-rinse product sprayed onto a microfiber cloth, do not spray directly on floor.

A few tips:

* Sweep, vacuum or dust mop regularly as dirt, abrasive and non abrasive, are the most common threat to your floor. Vacuum using air suction only
* Periodically clean the floor with a PH neutral cleaner made for laminate floors
* Remove spills/liquids immediately using a soft and absorbent cloth. Any spills left for an extended amount of time can cause damage to your floor
* Never wet-mop or flood your floor with water or other products. Only water-resistant laminate can be wet-mopped
* Maintain humidity in the home to prevent warping
* Only use floor cleaner’s specific to laminate. Do not use cleaners for ceramic, vinyl etc.
* Keep pet nails trimmed and free of dirt
* Do not use household cleaners, oils, waxes etc. on floor. This will cause a build-up and can damage your floor