

**Sheet Vinyl Maintenance**

Make sure the room is kept at a constant temperature for 48 hours after install to assure adhesive bonding (ex. If heat is turned off the floor will not adhere). Avoid any heavy cleaning or scrubbing for 3 days after install. Try to avoid heavy traffic for 48 hours to allow floor to set.

A few tips:

* Wipe spills up as soon as they occur. Use a neutral PH cleaner once the floor has dried
* Sweep or vacuum regularly. Avoid vacuums with a beater bar as it will damage your floor
* Damp mop using a clean mop or cloth. Frequently rinse in clean water
* When necessary, mop the floor with a solution of clean water and mild detergent or domestic floor cleaning emulsion (do not use polish, liquid/powder abrasive cleaners, bleach or strong detergents)
* Do not drag heavy appliances or furniture across floor, this can cause the flooring to tear or dent